CARD SORT: Category Cards

|  |  |
| --- | --- |
| **ISO** | **Shutter Speed** |
| **Aperture** | **Mirrorless Camera** |
| **DSLR** | **Camcorder** |
| **Webcam** | **[P] Program Mode** |
| **[Av] Aperture Priority** | **[Tv] Shutter Priority** |
| **[M] Manual** |  |

CARD SORT: Sorting Cards

|  |  |
| --- | --- |
|  The camera automatically sets up both the aperture and the shutter speed. | You set the aperture in f-stops while the camera sets the shutter speed. |
| You set the shutter speed while the camera sets the aperture in f-stops. | You will have complete control of all your exposure settings. |
| Represents the sensitivity of the camera’s image sensor to light | How long a single image is exposed to the outside light |
| (or F-Stop) Regulates how much the lens will open up and let light into your sensor | A small, portable device that records video and sound. |
| A digital camera that uses a mirror to direct light onto a sensor to capture images. | A digital camera that captures images without a reflex mirror. Rather, light passes directly from the lens to a digital sensor, which then displays the image on the camera’s screen.  |
| A video camera that is connected to a computer or integrated in a device and allows its images to be seen online |  |