CARD SORT: LABEL CARDS

|  |  |
| --- | --- |
| **Lens** | **Work piece** |
| **Laser** | **Cutting gas inlet** |
| **Mirror** | **Output Nozzle** |
| **Flight tube** | **Lens mount** |

CARD SORT: FUNCTION CARDS

|  |  |
| --- | --- |
| Focuses the beam to a small precise point. | Serves as the cutting element. |
| Directs the laser beam where it needs to go. | Protects the laser beam path and maintains alignment. |
| This is where the laser actually leaves the cutter. | Supplies gas to cool the material and enhance cutting efficiency. |
| This is the piece you are actually cutting with the laser. | The component that keeps the lens in place. |